SECTION 11 6500

**PART 1 - GENERAL**

1.01SUMMARY

 A. This section may include, but is not limited to the following track & field equipment:

 1. 16” Adjustable **Take Off Board System**

B. Related Sections: Review Contract Documents for requirements that affect work of this section. Specification sections that directly relate to work of this section include, but are not limited to:

        Section 33 3000 – Site Improvements

Section 32 1826 - Synthetic Grass Surfacing

        Section 32 1822 – Synthetic Athletic & Sports Surfacing

        Section 12 9300 – Site Furnishings

        Section 03 3000 – Cast-in-Place Concrete

Section 11 6500 – Athletic & Recreational Equipment

1.02 SUBMITTALS

A. Product Data: Submit manufacturer’s product literature, technical specifications, and other data required to demonstrate compliance with specified requirements for all athletic equipment.

1.03 QUALITY ASSURANCE

A. Fabrication and installation of site improvements by experienced craftsmen with excellent record of performance on completed projects of comparable size, scope, and quality.

 B. All materials, hardware and furnishings shall be new, first quality.

1.04 FIELD MEASUREMENTS

A. Contractor shall verify position and layout of track and field equipment. Verify dimensions by field measurements.

**PART 2 - PRODUCTS**

2.01 MANUFACTURERS

A. Manufacturers and product selections named are provided to establish the minimum standard and shall comply with NFHS requirements. Equipment shall be as manufactured by:

**SportsEdge®**

P.O. Box 837, 259 Murdock Rd.

Troutman, NC 28166

P: 800-334-6057

Fax: 704-528-0179

info@sportsedge.com

www.sportsedge.com

 B. Substitutions: Requests for substitutions will be considered in accordance with Section 01630.

2.2 LONG JUMP & TRIPLE JUMP TAKE-OFF BOARD SYSTEMS

 A. Long Jump & Triple Jump Take-Off Board Systems: **Model No. SE446** Take-Off Board System.

1. Aluminum Tray: Constructed of 3/16” thick aluminum, formed and welded.

1. Aluminum Base Board: Constructed of 1/8” aluminum sheet, formed to shape. All adjustment screws are stainless steel. The base board can be adjusted for level and height, using six adjustment screws, without removing the base board from the tray. There are six threaded fasteners for attaching the take-off board.
2. Wood Take-Off Board: Constructed of ¾” marine grade plywood with a white outdoor enamel coating. There are six counter-sunk holes for mounting to the base board. The take-off board is finished on both sides so that it can be reversible.

**PART 3 - EXECUTION**

3.03 INSTALLATION

A. All athletic equipment shall be installed as recommended by manufacturer's written directions, and as indicated on the drawings.

-- END OF SECTION --