SECTION 11 6823

**PART 1 GENERAL**

* 1. RELATED WORK

Review Contract Documents for requirements that affect work of this section. Specification sections that directly relate to work of this section include, but are not limited to:

        Section [11 6500 - Athletic & Recreational Equipment](http://www.4specs.com/s/11/11480.html)

Section 12 9300 - Site Furnishings

Section 31 2300 - Excavation and Fill

Section 33 3000 - Site Improvements

Section 32 1820 - Athletic & Sports Surfaces

Section 32 1826 - Synthetic Grass Surfacing

Section 32 9200 -Turf and Grasses

1.02 SUBMITTALS

A. Product Data: Submit manufacturer’s product literature, technical specifications, and other data required to demonstrate compliance with specified requirements for all athletic equipment.

1.03 QUALITY ASSURANCE

A. Fabrication and installation of site improvements by experienced craftsmen with excellent record of performance on completed projects of comparable size, scope, and quality.

B. All materials, hardware and furnishings shall be new, first quality.

1.04 FIELD MEASUREMENTS

A. Contractor shall verify position and layout of rubber border. Verify dimensions by field measurements.

* 1. SYSTEM DESCRIPTION

1. Rubber Border System for Beach Volleyball; Rubber Curb with rounded top, 8.5”W x 9.75"H x 96"L, shall be manufactured of 100% recycled rubber, assembly number SEFLEXVBC-SM, Small Court 72’ 3”’ x 41’3”.

**PART 2 PRODUCTS**

2.01 FlexEdge® Rubber Curb

A. Base: Model **#SEFLEXVBC-SM** (Small Court 72’ 3”’ x 41’3”) by:

SportsEdge®

259 Murdock Rd.

Troutman, NC 28166

PH: 800-334-6057

FX: 704-528-0179

info@sportsedge.com

www.sportsedge.com

B. COMPONENTS: Beach Volleyball Rubber Border System for small court size meeting the following criteria as the minimum standard:

1. Rubber Curb:

a. 8.5”W x 9.75"H x 96"L

b. Manufactured of 100% premium grade recycled rubber from truck

tires  
c. Manufactured of 90% post-consumer content

2. Pre-fabricated Corners:

a. 8.5”W x 9.75"H x 13.5”L each side

b. Manufactured of 100% premium grade recycled rubber from truck

tires   
c. Manufactured of 90% post-consumer content

3. Accessories:

1. 18” Anchor Pins, Steel w/ welded cap, part # SEFLEXA18
2. Betaseal Adhesive, 10.5 oz., part # SEFLEXBST
3. UV Top Coat - 4 Liter, part # SEFLEXTC

**PART 3 EXECUTION**

3.01 INSTALLATION OF EQUIPMENT

A. Install as recommended by the manufacturer, and as indicated on the drawings. The installing contractor shall ensure that the base is compacted and level to correct elevation.

END OF SECTION