SECTION 11 6500

**PART 1 - GENERAL**

1.01SUMMARY

A. This section may include, but is not limited to the following track & field equipment:

1. **16” Synthetic Adjustable Take Off Board System Model No. SE446S**

B. Related Sections: Review Contract Documents for requirements that affect work of this section. Specification sections that directly relate to work of this section include, but are not limited to:

        Section 33 3000 – Site Improvements

Section 32 1826 - Synthetic Grass Surfacing

        Section 32 1822 – Synthetic Athletic & Sports Surfacing

        Section 12 9300 – Site Furnishings

        Section 03 3000 – Cast-in-Place Concrete

Section 11 6500 – Athletic & Recreational Equipment

1.02 SUBMITTALS

A. Product Data: Submit manufacturer’s product literature, technical specifications, and other data required to demonstrate compliance with specified requirements for all athletic equipment.

1.03 QUALITY ASSURANCE

A. Fabrication and installation of site improvements by experienced craftsmen with excellent record of performance on completed projects of comparable size, scope, and quality.

B. All materials, hardware and furnishings shall be new, first quality.

1.04 FIELD MEASUREMENTS

A. Contractor shall verify position and layout of track and field equipment. Verify dimensions by field measurements.

**PART 2 - PRODUCTS**

2.01 MANUFACTURERS

A. Manufacturers and product selections named are provided to establish the minimum standard and shall comply with NFHS requirements. Equipment shall be as manufactured by:

**SportsEdge®**

259 Murdock Rd.

Troutman, NC 28166

Phone: 800-334-6057

info@sportsedge.com

www.sportsedge.com

B. Substitutions: Requests for substitutions will be considered in accordance with Section 01630.

2.2 LONG JUMP & TRIPLE JUMP TAKE-OFF BOARD SYSTEMS

A. Long Jump & Triple Jump Take-Off Board Systems: **Model No. SE446S** Take-Off Board System.

The base board can be fully adjusted for level and height using six adjustment screws with four threaded fasteners for attaching the take-off board. Spline plates must retain the synthetic take off board continuously along each 48” long edge. The synthetic take off system shall have the following attributes:

1. Aluminum Tray - 0.190" Thick 5052-H32 Aluminum, Welded Assembly

2. Leveling Base - 0.125" Thick 5052-H32 Aluminum

3. Spline Plates - 0.100" Thick 5052-H32 Aluminum

4. Fasteners - Type 304 Stainless Steel

5. Synthetic Take-Off Board

* 1. Dimensions: 1” Thick x 16” W x 48” L
  2. Surface: Slightly Textured Surface
  3. Color: White

**PART 3 - EXECUTION**

3.03 INSTALLATION

A. All athletic equipment shall be installed as recommended by manufacturer's written directions, and as indicated on the drawings.

-- END OF SECTION --