SECTION 03 1000

**PART 1 GENERAL**

* 1. RELATED WORK

Review Contract Documents for requirements that affect work of this section. Specification sections that directly relate to work of this section include, but are not limited to:

        Section 03 10000 – Concrete Forming and Accessories

 Section [11 6500 - Athletic & Recreational Equipment](http://www.4specs.com/s/11/11480.html)

 Section 12 9300 - Site Furnishings

Section 31 2300 - Excavation and Fill

Section 33 3000 - Site Improvements

Section 32 1820 - Athletic & Sports Surfaces

Section 32 1826 - Synthetic Grass Surfacing

Section 32 9200 -Turf and Grasses

1.02 SUBMITTALS

A. Product Data: Submit manufacturer’s product literature, technical specifications, and other data required to demonstrate compliance with specified requirements for all athletic equipment.

1.03 QUALITY ASSURANCE

A. Fabrication and installation of site improvements by experienced craftsmen with excellent record of performance on completed projects of comparable size, scope, and quality.

 B. All materials, hardware and furnishings shall be new, first quality.

1.04 FIELD MEASUREMENTS

A. Contractor shall verify position and layout of rubber border. Verify dimensions by field measurements.

* 1. SYSTEM DESCRIPTION
1. Rubber Curb Cap for application to the top of a cast-in-place or pre-cast concrete curb, Model # **SEFLEXCC** and **SEFLEXCC.8** (*Specifier Select)*

**PART 2 PRODUCTS**

2.01 FlexEdge® Rubber Curb Cap

A. Base: Model # **SEFLEXCC** and **SEFLEXCC.8** by:

SportsEdge®

259 Murdock Rd.

Troutman, NC 28166

PH: 800-334-6057

FX: 704-528-0179

info@sportsedge.com

www.sportsedge.com

B. COMPONENTS: *(Specifier Select 1 or 2)*

1. Rubber Curb Cap SEFLEXCC:

a. 6” W x 96” l x 2” H with chamfered corners

b. Manufactured of 100% premium grade recycled rubber from truck

 tires
c. Manufactured of 90% post-consumer content

2. Rubber Curb Cap SEFLEXCC.8:

a. 8” W x 96” l x 2” H with chamfered corners

b. Manufactured of 100% premium grade recycled rubber from truck

 tires
c. Manufactured of 90% post-consumer content

3. Accessories:

1. Betaseal Adhesive, 10.5 oz., part # SEFLEXBST
2. UV Top Coat - 4 Liter, part # SEFLEXTC

**PART 3 EXECUTION**

3.01 INSTALLATION OF EQUIPMENT

A. Install as recommended by the manufacturer, and as indicated on the drawings. The installing contractor shall ensure that the base is compacted and level to correct elevation.

END OF SECTION