SECTION 11 6833

**PART 1 GENERAL**

* 1. RELATED WORK

Review Contract Documents for requirements that affect work of this section. Specification sections that directly relate to work of this section include, but are not limited to:

        Section 33 3000 – Site Improvements

Section 32 1826 - Synthetic Grass Surfacing

        Section 32 1822 – Synthetic Athletic & Sports Surfacing

        Section 12 9300 – Site Furnishings

        Section 03 3000 – Cast-in-Place Concrete

Section 11 6500 – Athletic & Recreational Equipment

1.02 SUBMITTALS

A. Product Data: Submit manufacturer’s product literature, technical specifications, and other data required to demonstrate compliance with specified requirements for all athletic equipment.

1.03 QUALITY ASSURANCE

A. Fabrication and installation of site improvements by experienced craftsmen with excellent record of performance on completed projects of comparable size, scope, and quality.

 B. All materials, hardware and furnishings shall be new, first quality.

1.04 FIELD MEASUREMENTS

A. Contractor shall verify position and layout of all athletic field equipment. Verify dimensions by field measurements.

* 1. SYSTEM DESCRIPTION

A. 12” Wood IAAF Take Off Board Model #**SE43501.**

**PART 2 - PRODUCTS**

 2.01 MANUFACTURERS

 A. Manufacturers and product selections named are provided to establish the minimum standard and shall comply with NFHS and NCAA requirements. Equipment shall be as manufactured by:

SportsEdge®

P.O. Box 837

259 Murdock Rd.

Troutman, NC 28166

PH: 800-334-6057

FX: 704-528-0179

info@sportsedge.com

www.sportsedge.com

 2.02 LONG/TRIPLE JUMP TAKE-OFF BOARD SYSTEMS

 A. 12” Wood IAAF Long/Triple Jump Take-Off Board System: **Model #SE43501**

 1. Aluminum Tray: Constructed of 3/16” thick aluminum, formed and welded.

 2. Aluminum Base Board: Constructed of 1/8” aluminum sheet (3003), formed to

 shape. All adjustment screws are stainless steel. The base board can be adjusted

 for level and height, using six adjustment screws, without removing the base board

 from the tray. There are four threaded fasteners for attaching the take-off board.

 3. 12” Wood Take-Off Board: Constructed of ¾” A/B marine grade plywood with a white outdoor enamel coating. Shall have four counter-sunk holes for mounting to the base board. The take-off board is finished on both sides to make it reversible.

**PART 3 - EXECUTION**

 3.03 INSTALLATION

 A. All athletic equipment shall be installed as recommended by manufacturer's written directions, and as indicated on the drawings.

END OF SECTION