SECTION 11 6500

PART 1 – GENERAL

1.01 SUMMARY

 A. This section may include, but is not limited to the following track & field equipment:

 1. **Outdoor Volleyball System**

B. Related Sections: Review Contract Documents for requirements that affect work of this section. Specification sections that directly relate to work of this section include, but are not limited to:

        Section 33 3000 – Site Improvements

Section 32 1826 - Synthetic Grass Surfacing

        Section 32 1822 – Synthetic Athletic & Sports Surfacing

        Section 12 9300 – Site Furnishings

        Section 03 3000 – Cast-in-Place Concrete

Section 11 6500 – Athletic & Recreational Equipment

1.02 SUBMITTALS

A. Product Data: Submit manufacturer’s product literature, technical specifications, and other data required to demonstrate compliance with specified requirements for all athletic equipment.

1.03 QUALITY ASSURANCE

A. Fabrication and installation of site improvements by experienced craftsmen with excellent record of performance on completed projects of comparable size, scope, and quality.

 B. All materials, hardware and furnishings shall be new, first quality.

1.04 FIELD MEASUREMENTS

A. Contractor shall verify position and layout of track and field equipment. Verify dimensions by field measurements.

PART 2 - PRODUCTS

2.01 MANUFACTURERS

A. Manufacturers and product selections named are provided to establish the minimum standard and shall comply with the safety standards as outlined below (2.02B).

Equipment shall be as supplied by:

SportsEdge®

259 Murdock Rd.

Troutman, NC 28166

PH: 800-334-6057

www.sportsedge.com

info@sportsedge.com

 B. Substitutions: Requests for substitutions will be considered in accordance with Section 01630 (01 25 13).

2.02 ATHLETIC EQUIPMENT

 A. General: Model SEOCV-900 Outdoor volleyball system with the following attributes:

1. Constructed of 3-1/2" galvanized steel tubing

2. Powder coated uprights with fixed net height strap roller bearings positioned for official men's and women's competition heights

3. Rust resistant positive lock ratchet net tensioning device

4. 36" aluminum ground sleeves with cast aluminum top caps for semi-permanent installation

5. NET- Model SEPVBN-6J

PART 3: EXECUTION

3.03 INSTALLATION

A. All athletic equipment shall be installed as recommended by manufacturer's written directions, and as indicated on the drawings.

-- END OF SECTION --